<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<packages>
<package name="ACQUA">
<description>ACQUA- from Acmesystems.it</description>
</package>
</packages>
<symbols>
<symbol name="ACQUA">
<description>J1 = left side
J2 = bottom side
J3 = right side</description>
<pin name="ETH_TXP"/>
<pin name="ETH_RXN"/>
<pin name="ETH_TXN"/>
<pin name="ETH_RXP"/>
<pin name="ETH_GND"/>
<pin name="ETH_3V3"/>
<pin name="ETH_LED1"/>
<pin name="ETH_LED2"/>
<pin name="LCD_DAT1"/>
<pin name="LCD_DAT0"/>
<pin name="LCD_DAT3"/>
<pin name="LCD_DAT2"/>
<pin name="LCD_DAT5"/>
<pin name="LCD_DAT4"/>
<pin name="LCD_DAT7"/>
<pin name="LCD_DAT6"/>
<pin name="LCD_DAT9"/>
<pin name="LCD_DAT8"/>
<pin name="LCD_DAT11"/>
<pin name="LCD_DAT10"/>
<pin name="LCD_DAT13"/>
<pin name="LCD_DAT12"/>
<pin name="LCD_DAT15"/>
<pin name="LCD_DAT14"/>
<pin name="LCD_DAT17"/>
<pin name="LCD_DAT16"/>
<pin name="LCD_DAT19"/>
<pin name="LCD_DAT18"/>
<pin name="LCD_DAT21"/>
<pin name="LCD_DAT20"/>
<pin name="LCD_DAT23"/>
<pin name="LCD_DAT22"/>
<pin name="LCD_DSP"/>
<pin name="GND"/>
<pin name="LCD_HSYNC"/>
<pin name="LCD_PCK"/>
<pin name="LCD_DEN"/>
<pin name="LCD_VSYNC"/>
<pin name="LCD_PWM"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="AD2" direction="in"/>
<pin name="AD3" direction="in"/>
<pin name="AD4" direction="in"/>
<pin name="AD5" direction="in"/>
<pin name="AD6" direction="in"/>
<pin name="AD7" direction="in"/>
<pin name="AD8" direction="in"/>
<pin name="AD9" direction="in"/>
<pin name="ADVREF"/>
<pin name="AD11" direction="in"/>
<pin name="AD10" direction="in"/>
<pin name="A/D_TRIGGER"/>
<pin name="GND1"/>
<pin name="SPI0_CS0"/>
<pin name="SPI0_CK"/>
<pin name="SPI0_MOSI"/>
<pin name="SPI0_MISO"/>
<pin name="CTS0"/>
<pin name="SPI0_CS1"/>
<pin name="RXD0"/>
<pin name="RTS0"/>
<pin name="GPIO34"/>
<pin name="TXD0"/>
<pin name="GPIO38"/>
<pin name="GPIO35"/>
<pin name="GPIO39"/>
<pin name="GPIO43"/>
<pin name="GPIO42"/>
<pin name="USBA_P"/>
<pin name="3V3"/>
<pin name="USBA_N"/>
<pin name="GPIO36"/>
<pin name="USBB_P"/>
<pin name="GPIO37"/>
<pin name="USBB_N"/>
<pin name="GND2"/>
<pin name="USBC_P"/>
<pin name="GPIO32"/>
<pin name="USBC_N"/>
<pin name="GPIO33"/>
<pin name="GPIO46"/>
<pin name="GPIO40"/>
<pin name="GPIO47"/>
<pin name="GPIO41"/>
<pin name="GPIO48"/>
<pin name="GPIO44"/>
<pin name="GPIO49"/>
<pin name="GPIO45"/>
<pin name="GPIO50"/>
<pin name="GND3"/>
<pin name="RTS1"/>
<pin name="CTS1"/>
<pin name="GPIO57"/>
<pin name="RXD1"/>
<pin name="TXD1"/>
<pin name="WAKE_UP"/>
<pin name="SHUTDOWN"/>
<pin name="POWER_EN"/>
<pin name="NRST"/>
<pin name="BOOT_OFF"/>
<pin name="VBAT"/>
<pin name="DRXD"/>
<pin name="DTXD"/>
<pin name="RTS3"/>
<pin name="CTS3"/>
<pin name="TXD3"/>
<pin name="RXD3"/>
<pin name="GPIO143"/>
<pin name="CTS2"/>
<pin name="RTS2"/>
<pin name="RXD2"/>
<pin name="TXD2"/>
<pin name="GPIO148"/>
<pin name="MCI1_DA2"/>
<pin name="MCI1_DA3"/>
<pin name="MCI1_CDA"/>
<pin name="MCI1_DA1"/>
<pin name="MCI1_CK"/>
<pin name="MCI1_DA0"/>
<pin name="3V3_1"/>
<pin name="SPI1_MOSI"/>
<pin name="SPI1_CS0"/>
<pin name="SPI1_MISO"/>
<pin name="SPI1_CK"/>
<pin name="SPI1_CS1"/>
<pin name="GND4"/>
<pin name="SPI1_CS2"/>
<pin name="SPI1_CS3"/>
<pin name="UTXD0"/>
<pin name="URXD0"/>
<pin name="GPIO95"/>
<pin name="GPIO17"/>
<pin name="GPIO16"/>
<pin name="I2C_2_SLC"/>
<pin name="I2C_2_SDA"/>
<pin name="GPIO21"/>
<pin name="GPIO20"/>
<pin name="GPIO23"/>
<pin name="GPIO22"/>
<pin name="I2C_0_SLC"/>
<pin name="I2C_0_SDA"/>
<pin name="GPIO159"/>
<pin name="GPIO157"/>
<pin name="SSC_TK0"/>
<pin name="SSC_TF0"/>
<pin name="SSC_TD0"/>
<pin name="SSC_RK0"/>
<pin name="SSC_RF0"/>
<pin name="SSC_RD0"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ACQUA" prefix="ETH_TXP">
<gates>
<gate name="G$1" symbol="ACQUA"/>
</gates>
<devices>
<device name="ACQUA_A5" package="ACQUA">
<connects>
<connect gate="G$1" pin="3V3" pad="P$71"/>
<connect gate="G$1" pin="3V3_1" pad="P$121"/>
<connect gate="G$1" pin="A/D_TRIGGER" pad="P$53"/>
<connect gate="G$1" pin="AD0" pad="P$40"/>
<connect gate="G$1" pin="AD1" pad="P$41"/>
<connect gate="G$1" pin="AD10" pad="P$52"/>
<connect gate="G$1" pin="AD11" pad="P$51"/>
<connect gate="G$1" pin="AD2" pad="P$42"/>
<connect gate="G$1" pin="AD3" pad="P$43"/>
<connect gate="G$1" pin="AD4" pad="P$44"/>
<connect gate="G$1" pin="AD5" pad="P$45"/>
<connect gate="G$1" pin="AD6" pad="P$46"/>
<connect gate="G$1" pin="AD7" pad="P$47"/>
<connect gate="G$1" pin="AD8" pad="P$48"/>
<connect gate="G$1" pin="AD9" pad="P$49"/>
<connect gate="G$1" pin="ADVREF" pad="P$50"/>
<connect gate="G$1" pin="BOOT_OFF" pad="P$101"/>
<connect gate="G$1" pin="CTS0" pad="P$59"/>
<connect gate="G$1" pin="CTS1" pad="P$93"/>
<connect gate="G$1" pin="CTS2" pad="P$110"/>
<connect gate="G$1" pin="CTS3" pad="P$106"/>
<connect gate="G$1" pin="DRXD" pad="P$103"/>
<connect gate="G$1" pin="DTXD" pad="P$104"/>
<connect gate="G$1" pin="ETH_3V3" pad="P$6" route="any"/>
<connect gate="G$1" pin="ETH_GND" pad="P$5"/>
<connect gate="G$1" pin="ETH_LED1" pad="P$7"/>
<connect gate="G$1" pin="ETH_LED2" pad="P$8"/>
<connect gate="G$1" pin="ETH_RXN" pad="P$2"/>
<connect gate="G$1" pin="ETH_RXP" pad="P$4"/>
<connect gate="G$1" pin="ETH_TXN" pad="P$3"/>
<connect gate="G$1" pin="ETH_TXP" pad="P$1"/>
<connect gate="G$1" pin="GND" pad="P$34"/>
<connect gate="G$1" pin="GND1" pad="P$54"/>
<connect gate="G$1" pin="GND2" pad="P$77"/>
<connect gate="G$1" pin="GND3" pad="P$91"/>
<connect gate="G$1" pin="GND4" pad="P$127"/>
<connect gate="G$1" pin="GPIO143" pad="P$109"/>
<connect gate="G$1" pin="GPIO148" pad="P$114"/>
<connect gate="G$1" pin="GPIO157" pad="P$144"/>
<connect gate="G$1" pin="GPIO159" pad="P$143"/>
<connect gate="G$1" pin="GPIO16" pad="P$134"/>
<connect gate="G$1" pin="GPIO17" pad="P$133"/>
<connect gate="G$1" pin="GPIO20" pad="P$138"/>
<connect gate="G$1" pin="GPIO21" pad="P$137"/>
<connect gate="G$1" pin="GPIO22" pad="P$140"/>
<connect gate="G$1" pin="GPIO23" pad="P$139"/>
<connect gate="G$1" pin="GPIO32" pad="P$79"/>
<connect gate="G$1" pin="GPIO33" pad="P$81"/>
<connect gate="G$1" pin="GPIO34" pad="P$63"/>
<connect gate="G$1" pin="GPIO35" pad="P$66"/>
<connect gate="G$1" pin="GPIO36" pad="P$73"/>
<connect gate="G$1" pin="GPIO37" pad="P$75"/>
<connect gate="G$1" pin="GPIO38" pad="P$65"/>
<connect gate="G$1" pin="GPIO39" pad="P$67"/>
<connect gate="G$1" pin="GPIO40" pad="P$83"/>
<connect gate="G$1" pin="GPIO41" pad="P$85"/>
<connect gate="G$1" pin="GPIO42" pad="P$69"/>
<connect gate="G$1" pin="GPIO43" pad="P$68"/>
<connect gate="G$1" pin="GPIO44" pad="P$87"/>
<connect gate="G$1" pin="GPIO45" pad="P$89"/>
<connect gate="G$1" pin="GPIO46" pad="P$82"/>
<connect gate="G$1" pin="GPIO47" pad="P$84"/>
<connect gate="G$1" pin="GPIO48" pad="P$86"/>
<connect gate="G$1" pin="GPIO49" pad="P$88"/>
<connect gate="G$1" pin="GPIO50" pad="P$90"/>
<connect gate="G$1" pin="GPIO57" pad="P$94"/>
<connect gate="G$1" pin="GPIO95" pad="P$132"/>
<connect gate="G$1" pin="I2C_0_SDA" pad="P$142"/>
<connect gate="G$1" pin="I2C_0_SLC" pad="P$141"/>
<connect gate="G$1" pin="I2C_2_SDA" pad="P$136"/>
<connect gate="G$1" pin="I2C_2_SLC" pad="P$135"/>
<connect gate="G$1" pin="LCD_DAT0" pad="P$10"/>
<connect gate="G$1" pin="LCD_DAT1" pad="P$9"/>
<connect gate="G$1" pin="LCD_DAT10" pad="P$20"/>
<connect gate="G$1" pin="LCD_DAT11" pad="P$19"/>
<connect gate="G$1" pin="LCD_DAT12" pad="P$22"/>
<connect gate="G$1" pin="LCD_DAT13" pad="P$21"/>
<connect gate="G$1" pin="LCD_DAT14" pad="P$24"/>
<connect gate="G$1" pin="LCD_DAT15" pad="P$23"/>
<connect gate="G$1" pin="LCD_DAT16" pad="P$26"/>
<connect gate="G$1" pin="LCD_DAT17" pad="P$25"/>
<connect gate="G$1" pin="LCD_DAT18" pad="P$28"/>
<connect gate="G$1" pin="LCD_DAT19" pad="P$27"/>
<connect gate="G$1" pin="LCD_DAT2" pad="P$12"/>
<connect gate="G$1" pin="LCD_DAT20" pad="P$30"/>
<connect gate="G$1" pin="LCD_DAT21" pad="P$29"/>
<connect gate="G$1" pin="LCD_DAT22" pad="P$32"/>
<connect gate="G$1" pin="LCD_DAT23" pad="P$31"/>
<connect gate="G$1" pin="LCD_DAT3" pad="P$11"/>
<connect gate="G$1" pin="LCD_DAT4" pad="P$14"/>
<connect gate="G$1" pin="LCD_DAT5" pad="P$13"/>
<connect gate="G$1" pin="LCD_DAT6" pad="P$16"/>
<connect gate="G$1" pin="LCD_DAT7" pad="P$15"/>
<connect gate="G$1" pin="LCD_DAT8" pad="P$18"/>
<connect gate="G$1" pin="LCD_DAT9" pad="P$17"/>
<connect gate="G$1" pin="LCD_DEN" pad="P$37"/>
<connect gate="G$1" pin="LCD_DSP" pad="P$33"/>
<connect gate="G$1" pin="LCD_HSYNC" pad="P$35"/>
<connect gate="G$1" pin="LCD_PCK" pad="P$36"/>
<connect gate="G$1" pin="LCD_PWM" pad="P$39"/>
<connect gate="G$1" pin="LCD_VSYNC" pad="P$38"/>
<connect gate="G$1" pin="MCI1_CDA" pad="P$117"/>
<connect gate="G$1" pin="MCI1_CK" pad="P$119"/>
<connect gate="G$1" pin="MCI1_DA0" pad="P$120"/>
<connect gate="G$1" pin="MCI1_DA1" pad="P$118"/>
<connect gate="G$1" pin="MCI1_DA2" pad="P$115"/>
<connect gate="G$1" pin="MCI1_DA3" pad="P$116"/>
<connect gate="G$1" pin="NRST" pad="P$100"/>
<connect gate="G$1" pin="POWER_EN" pad="P$99"/>
<connect gate="G$1" pin="RTS0" pad="P$62"/>
<connect gate="G$1" pin="RTS1" pad="P$92"/>
<connect gate="G$1" pin="RTS2" pad="P$111"/>
<connect gate="G$1" pin="RTS3" pad="P$105"/>
<connect gate="G$1" pin="RXD0" pad="P$61"/>
<connect gate="G$1" pin="RXD1" pad="P$95"/>
<connect gate="G$1" pin="RXD2" pad="P$112"/>
<connect gate="G$1" pin="RXD3" pad="P$108"/>
<connect gate="G$1" pin="SHUTDOWN" pad="P$98"/>
<connect gate="G$1" pin="SPI0_CK" pad="P$56"/>
<connect gate="G$1" pin="SPI0_CS0" pad="P$55"/>
<connect gate="G$1" pin="SPI0_CS1" pad="P$60"/>
<connect gate="G$1" pin="SPI0_MISO" pad="P$58"/>
<connect gate="G$1" pin="SPI0_MOSI" pad="P$57"/>
<connect gate="G$1" pin="SPI1_CK" pad="P$125"/>
<connect gate="G$1" pin="SPI1_CS0" pad="P$123"/>
<connect gate="G$1" pin="SPI1_CS1" pad="P$126"/>
<connect gate="G$1" pin="SPI1_CS2" pad="P$128"/>
<connect gate="G$1" pin="SPI1_CS3" pad="P$129"/>
<connect gate="G$1" pin="SPI1_MISO" pad="P$124"/>
<connect gate="G$1" pin="SPI1_MOSI" pad="P$122"/>
<connect gate="G$1" pin="SSC_RD0" pad="P$150"/>
<connect gate="G$1" pin="SSC_RF0" pad="P$149"/>
<connect gate="G$1" pin="SSC_RK0" pad="P$148"/>
<connect gate="G$1" pin="SSC_TD0" pad="P$147"/>
<connect gate="G$1" pin="SSC_TF0" pad="P$146"/>
<connect gate="G$1" pin="SSC_TK0" pad="P$145"/>
<connect gate="G$1" pin="TXD0" pad="P$64"/>
<connect gate="G$1" pin="TXD1" pad="P$96"/>
<connect gate="G$1" pin="TXD2" pad="P$113"/>
<connect gate="G$1" pin="TXD3" pad="P$107"/>
<connect gate="G$1" pin="URXD0" pad="P$131"/>
<connect gate="G$1" pin="USBA_N" pad="P$72"/>
<connect gate="G$1" pin="USBA_P" pad="P$70"/>
<connect gate="G$1" pin="USBB_N" pad="P$76"/>
<connect gate="G$1" pin="USBB_P" pad="P$74"/>
<connect gate="G$1" pin="USBC_N" pad="P$80"/>
<connect gate="G$1" pin="USBC_P" pad="P$78"/>
<connect gate="G$1" pin="UTXD0" pad="P$130"/>
<connect gate="G$1" pin="VBAT" pad="P$102"/>
<connect gate="G$1" pin="WAKE_UP" pad="P$97"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
