Home ·

# SAMA5D4Config QML Type

Contains configuration values for a SAMA5D4 device. More...

Import Statement: | import SAMBA.Device.SAMA5D4 3.2

- List of all members, including inherited members

## Properties

- extram : alias
- nandflash : alias
- sdmmc : alias
- serial : alias
- serialflash : alias

## Detailed Description

By default, no configuration values are set.

## Serial Console Configuration

The following serial console configurations are supported:

Instance | Peripheral | I/O Set | TX Pin
--- | --- | --- | ---
0 | DBGU | 1 | PB25A
1 | UART0 | 1 | PE30B
2 | UART1 | 1 | PC26C
3 | USART0 | 1 | PD13A
4 | USART1 | 1 | PD17A
5 | USART2 | 1 | PB5B
6 | USART3 | 1 | PE17B
7 | USART4 | 1 | PE27B

## External RAM

The following external RAM configurations are supported:

Preset | Type | Model | Size
--- | --- | --- | ---
0 | DDR2 | MT47H128M8 | 4x128MB
1 | DDR2 | MT47H64M16 | 128MB
2 | DDR2 | MT47H128M16 | 2x256MB
2 | LPDDR2 | MT42L128M16 | 2*256MB
8 | DDR2 | W971G16SG | 128MB
9 | DDR2 | W972GG6KB | 2*256MB

## SD/MMC Configuration

The following SD/MMC configurations are supported:

Instance | Peripheral | I/O Set | Bus Width
--- | --- | --- | ---
0 | HSMCI0 (Slot A) | 1 | 1-bit, 4-bit, 8-bit
0 | HSMCI0 (Slot B) | 2 | 1-bit, 4-bit
1 | HSMCI1 | 1 | 1-bit, 4-bit

The SD/MMC applet on SAMA5D4 does not support voltage switching, so the voltage configuration property is ignored.

### Pin List for SD/MMC Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PC4B | Clock
PC5B | Command
PC6B | Data 0 (bus width: 1-bit, 4-bit, 8-bit)
PC7B | Data 1 (bus width: 4-bit, 8-bit)
PC8B | Data 2 (bus width: 4-bit, 8-bit)
PC9B | Data 3 (bus width: 4-bit, 8-bit)
PC10B | Data 4 (bus width: 8-bit)
PC11B | Data 5 (bus width: 8-bit)
PC12B | Data 6 (bus width: 8-bit)
PC13B | Data 7 (bus width: 8-bit)

### Pin List for SD/MMC Instance 0 (I/O Set 2)

Pin | Use
--- | ---
PC4B | Clock
PE0B | Command
PE1B | Data 0 (bus width: 1-bit, 4-bit)
PE2B | Data 1 (bus width: 4-bit)
PE3B | Data 2 (bus width: 4-bit)
PE4B | Data 3 (bus width: 4-bit)

### Pin List for SD/MMC Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PE18C | Clock
PE19C | Command
PE20C | Data 0 (Bus Width: 1-bit, 4-bit)
PE21C | Data 1 (Bus Width: 4-bit)
PE22C | Data 2 (Bus Width: 4-bit)
PE23C | Data 3 (Bus Width: 4-bit)

## SPI Serial Flash Configuration

The following SPI Serial Flash configurations are supported:

Instance | Peripheral | I/O Set | Chip Selects
--- | --- | --- | ---
0 | SPI0 | 1 | 0, 1, 2, 3
0 | SPI0 | 2 | 1, 2
1 | SPI1 | 1 | 0, 1, 2, 3
1 | SPI1 | 2 | 1, 2, 3
2 | SPI2 | 1 | 0, 1, 2, 3

### Pin List for SPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PC0A | MISO
PC1A | MOSI
PC2A | SPCK
PC3A | NPCS0
PC4A | NPCS1
PC28B | NPCS2
PC29B | NPCS3

### Pin List for SPI Serial Flash Instance 0 (I/O Set 2)

Pin | Use
--- | ---
PC0A | MISO
PC1A | MOSI
PC2A | SPCK
PC27B | NPCS1
PD31A | NPCS2

### Pin List for SPI Serial Flash Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PB18A | MISO
PB19A | MOSI
PB20A | SPCK
PB21A | NPCS0
PA26C | NPCS1
PA27C | NPCS2
PA28C | NPCS3

### Pin List for SPI Serial Flash Instance 1 (I/O Set 2)

Pin | Use
--- | ---
PB18A | MISO
PB19A | MOSI
PB20A | SPCK
PB22A | NPCS1
PB23A | NPCS2
PB27A | NPCS3

### Pin List for SPI Serial Flash Instance 2 (I/O Set 1)

Pin | Use
--- | ---
PD11B | MISO
PD13B | MOSI
PD15B | SPCK
PD17B | NPCS0
PB14B | NPCS1
PB15B | NPCS2
PB28A | NPCS3

## NAND Flash Configuration

The following NAND Flash configurations are supported:

I/O Set | Bus Width
--- | ---
1 | 8-bit, 16-bit

### Pin List for NAND Flash (I/O Set 1)

Pin | Use | Bus Width
--- | --- | ---
PC13A | NANDOE | 8-bit, 16-bit
PC14A | NANDWE | 8-bit, 16-bit
PC15A | NCS3 | 8-bit, 16-bit
PC16A | NANDRDY | 8-bit, 16-bit
PC17A | NANDALE | 8-bit, 16-bit
PC18A | NANDCLE | 8-bit, 16-bit
PC5A | D0 | 8-bit, 16-bit
PC6A | D1 | 8-bit, 16-bit
PC7A | D2 | 8-bit, 16-bit
PC8A | D3 | 8-bit, 16-bit
PC9A | D4 | 8-bit, 16-bit
PC10A | D5 | 8-bit, 16-bit
PC11A | D6 | 8-bit, 16-bit
PC12A | D7 | 8-bit, 16-bit
PB18B | D8 | 16-bit
PB19B | D9 | 16-bit
PB20B | D10 | 16-bit
PB21B | D11 | 16-bit
PB22B | D12 | 16-bit
PB23B | D13 | 16-bit
PB24B | D14 | 16-bit
PB25B | D15 | 16-bit

## Property Documentation

extram : alias

Configuration for external RAM applet

See ExtRamConfig for a list of configurable properties.

nandflash : alias

Configuration for NAND Flash applet

See NANDFlashConfig for a list of configurable properties.

sdmmc : alias

Configuration for SD/MMC applet

See SDMMCConfig for a list of configurable properties.

serial : alias

Configuration for applet serial console output

See SerialConfig for a list of configurable properties.

serialflash : alias

Configuration for SPI Serial Flash applet

See SerialFlashConfig for a list of configurable properties.