Home ·

# SAMA5D3Config QML Type

Contains configuration values for a SAMA5D3 device. More...

Import Statement: | import SAMBA.Device.SAMA5D3 3.2

- List of all members, including inherited members

## Properties

- extram : alias
- nandflash : alias
- sdmmc : alias
- serial : alias
- serialflash : alias

## Detailed Description

By default, no configuration values are set.

## Serial Console Configuration

The following serial console configurations are supported:

Instance | Peripheral | I/O Set | TX Pin
--- | --- | --- | ---
0 | DBGU | 1 | PB31A
1 | UART0 | 1 | PC30A
2 | UART1 | 1 | PA31B
3 | USART0 | 1 | PD18A
4 | USART1 | 1 | PB29A
5 | USART2 | 1 | PE26B
6 | USART3 | 1 | PE19B

## External RAM

The following external RAM configurations are supported:

Preset | Type | Model | Size
--- | --- | --- | ---
0 | DDR2 | MT47H128M8 | 4x128MB
1 | DDR2 | MT47H64M16 | 128MB
2 | DDR2 | MT47H128M16 | 2x256MB
2 | LPDDR2 | MT42L128M16 | 2*256MB
8 | DDR2 | W971G16SG | 128MB
9 | DDR2 | W972GG6KB | 2*256MB

## SD/MMC Configuration

The following SD/MMC configurations are supported:

Instance | Peripheral | I/O Set | Bus Width
--- | --- | --- | ---
0 | HSMCI0 | 1 | 1-bit, 4-bit, 8-bit
1 | HSMCI1 | 1 | 1-bit, 4-bit
2 | HSMCI2 | 1 | 1-bit, 4-bit

The SD/MMC applet on SAMA5D3 does not support voltage switching, so the voltage configuration property is ignored.

### Pin List for SD/MMC Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PD9A | Clock
PD0A | Command
PD1A | Data 0 (bus width: 1-bit, 4-bit, 8-bit)
PD2A | Data 1 (bus width: 4-bit, 8-bit)
PD3A | Data 2 (bus width: 4-bit, 8-bit)
PD4A | Data 3 (bus width: 4-bit, 8-bit)
PD5A | Data 4 (bus width: 8-bit)
PD6A | Data 5 (bus width: 8-bit)
PD7A | Data 6 (bus width: 8-bit)
PD8A | Data 7 (bus width: 8-bit)

### Pin List for SD/MMC Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PB24A | Clock
PB19A | Command
PB20A | Data 0 (bus width: 1-bit, 4-bit)
PB21A | Data 1 (bus width: 4-bit)
PB22A | Data 2 (bus width: 4-bit)
PB23A | Data 3 (bus width: 4-bit)

### Pin List for SD/MMC Instance 2 (I/O Set 1)

Pin | Use
--- | ---
PC15A | Clock
PC10A | Command
PC11A | Data 0 (Bus Width: 1-bit, 4-bit)
PC12A | Data 1 (Bus Width: 4-bit)
PC13A | Data 2 (Bus Width: 4-bit)
PC14A | Data 3 (Bus Width: 4-bit)

## SPI Serial Flash Configuration

The following SPI Serial Flash configurations are supported:

Instance | Peripheral | I/O Set | Chip Selects
--- | --- | --- | ---
0 | SPI0 | 1 | 0, 1, 2, 3
1 | SPI1 | 1 | 0, 1, 2, 3

### Pin List for SPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PD10A | MISO
PD11A | MOSI
PD12A | SPCK
PD13A | NPCS0
PD14B | NPCS1
PD15B | NPCS2
PD16B | NPCS3

### Pin List for SPI Serial Flash Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PC22A | MISO
PC23A | MOSI
PC24A | SPCK
PC25A | NPCS0
PC26A | NPCS1
PC27A | NPCS2
PC28A | NPCS3

## NAND Flash Configuration

The following NAND Flash configurations are supported:

I/O Set | Bus Width
--- | ---
1 | 8-bit, 16-bit

### Pin List for NAND Flash (I/O Set 1)

Pin | Use | Bus Width
--- | --- | ---
PE21A | NANDALE | 8-bit, 16-bit
PE22A | NANDCLE | 8-bit, 16-bit

Other NAND pins are not muxed by the PIO controller.

## Property Documentation

extram : alias

Configuration for external RAM applet

See ExtRamConfig for a list of configurable properties.

nandflash : alias

Configuration for NAND Flash applet

See NANDFlashConfig for a list of configurable properties.

sdmmc : alias

Configuration for SD/MMC applet

See SDMMCConfig for a list of configurable properties.

serial : alias

Configuration for applet serial console output

See SerialConfig for a list of configurable properties.

serialflash : alias

Configuration for SPI Serial Flash applet

See SerialFlashConfig for a list of configurable properties.