Home ·

# SAMA5D2Config QML Type

Contains configuration values for a SAMA5D2 device. More...

Import Statement: | import SAMBA.Device.SAMA5D2 3.2

- List of all members, including inherited members

## Properties

- extram : alias
- nandflash : alias
- qspiflash : alias
- sdmmc : alias
- serial : alias
- serialflash : alias

## Detailed Description

By default, no configuration values are set.

## Serial Console Configuration

The following serial console configurations are supported:

Instance | Peripheral | I/O Set | TX Pin
--- | --- | --- | ---
0 | UART0 | 1 | PB27C
1 | UART1 | 1 | PD3A
1 | UART1 | 2 | PC8E
2 | UART2 | 1 | PD5B
2 | UART2 | 2 | PD24A
2 | UART2 | 3 | PD20C
3 | UART3 | 1 | PC13D
3 | UART3 | 2 | PD0C
3 | UART3 | 3 | PB12C
4 | UART4 | 1 | PB4A
5 | FLEXCOM0 | 1 | PB28C
6 | FLEXCOM1 | 1 | PA24A
7 | FLEXCOM2 | 1 | PA6E
7 | FLEXCOM2 | 2 | PD26C
8 | FLEXCOM3 | 1 | PA15E
8 | FLEXCOM3 | 2 | PC20E
8 | FLEXCOM3 | 3 | PB23E
9 | FLEXCOM4 | 1 | PC28B
9 | FLEXCOM4 | 2 | PD12B
9 | FLEXCOM4 | 3 | PD21C

## External RAM

The following external RAM configurations are supported:

Preset | Type | Model | Size
--- | --- | --- | ---
0 | DDR2 | MT47H128M8 | 4x128MB
1 | DDR2 | MT47H64M16 | 128MB
2 | DDR2 | MT47H128M16 | 2x256MB
2 | LPDDR2 | MT42L128M16 | 2*256MB
4 | DDR3 | MT41K128M16 | 2*256MB
5 | LPDDR3 | EDF8164A3MA | 2*256MB
8 | DDR2 | W971G16SG | 128MB
9 | DDR2 | W972GG6KB | 2*256MB

## SD/MMC Configuration

The following SD/MMC configurations are supported:

Instance | Peripheral | I/O Set | Bus Width | Voltage Switch Support
--- | --- | --- | --- | ---
0 | SDMMC0 | 1 | 1-bit, 4-bit, 8-bit | yes
1 | SDMMC1 | 1 | 1-bit, 4-bit | no

### Pin List for SD/MMC Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PA0A | Clock
PA1A | Command
PA2A | Data 0 (bus width: 1-bit, 4-bit, 8-bit)
PA3A | Data 1 (bus width: 4-bit, 8-bit)
PA4A | Data 2 (bus width: 4-bit, 8-bit)
PA5A | Data 3 (bus width: 4-bit, 8-bit)
PA6A | Data 4 (bus width: 8-bit)
PA7A | Data 5 (bus width: 8-bit)
PA8A | Data 6 (bus width: 8-bit)
PA9A | Data 7 (bus width: 8-bit)
PA11A | VDD Selection

### Pin List for SD/MMC Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PA22E | Clock
PA28E | Command
PA18E | Data 0 (bus width: 1-bit, 4-bit)
PA19E | Data 1 (bus width: 4-bit)
PA20E | Data 2 (bus width: 4-bit)
PA21E | Data 3 (bus width: 4-bit)

## SPI Serial Flash Configuration

The following SPI Serial Flash configurations are supported:

Instance | Peripheral | I/O Set | Chip Selects
--- | --- | --- | ---
0 | SPI0 | 1, 2 | 0, 1, 2, 3
1 | SPI1 | 1, 2 | 0, 1, 2, 3
1 | SPI1 | 3 | 0, 1, 2
2 | FLEXCOM0 | 1 | 0, 1
3 | FLEXCOM1 | 1 | 0, 1
4 | FLEXCOM2 | 1, 2 | 0, 1
5 | FLEXCOM3 | 1, 2, 3 | 0, 1
6 | FLEXCOM4 | 1, 2, 3 | 0, 1

### Pin List for SPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PA16A | MISO
PA15A | MOSI
PA14A | SPCK
PA17A | NPCS0
PA18A | NPCS1
PA19A | NPCS2
PA20A | NPCS3

### Pin List for SPI Serial Flash Instance 0 (I/O Set 2)

Pin | Use
--- | ---
PA31C | MISO
PB0C | MOSI
PB1C | SPCK
PA30C | NPCS0
PA29C | NPCS1
PA27C | NPCS2
PA28C | NPCS3

### Pin List for SPI Serial Flash Instance 1 (I/O Set 1)

Pin | Use
--- | ---
PC3D | MISO
PC2D | MOSI
PC1D | SPCK
PC4D | NPCS0
PC5D | NPCS1
PC6D | NPCS2
PC7D | NPCS3

### Pin List for SPI Serial Flash Instance 1 (I/O Set 2)

Pin | Use
--- | ---
PA24D | MISO
PA23D | MOSI
PA22D | SPCK
PA25D | NPCS0
PA26D | NPCS1
PA27D | NPCS2
PA28D | NPCS3

### Pin List for SPI Serial Flash Instance 1 (I/O Set 3)

Pin | Use
--- | ---
PD27A | MISO
PD26A | MOSI
PD25A | SPCK
PD28A | NPCS0
PD29A | NPCS1
PD30A | NPCS2

### Pin List for SPI Serial Flash Instance 2 (I/O Set 1)

Pin | Use
--- | ---
PC28C | MOSI
PC29C | MISO
PC30C | SPCK
PB31C | NPCS0
PC0C | NPCS1

### Pin List for SPI Serial Flash Instance 3 (I/O Set 1)

Pin | Use
--- | ---
PA24A | MOSI
PA23A | MISO
PA22A | SPCK
PA25A | NPCS0
PA26A | NPCS1

### Pin List for SPI Serial Flash Instance 4 (I/O Set 1)

Pin | Use
--- | ---
PA6E | MOSI
PA7E | MISO
PA8E | SPCK
PA9E | NPCS0
PA10E | NPCS1

### Pin List for SPI Serial Flash Instance 4 (I/O Set 2)

Pin | Use
--- | ---
PD26C | MOSI
PD27C | MISO
PD28C | SPCK
PD29C | NPCS0
PD30C | NPCS1

### Pin List for SPI Serial Flash Instance 5 (I/O Set 1)

Pin | Use
--- | ---
PA15E | MOSI
PA13E | MISO
PA14E | SPCK
PA16E | NPCS0
PA17E | NPCS1

### Pin List for SPI Serial Flash Instance 5 (I/O Set 2)

Pin | Use
--- | ---
PC20E | MOSI
PC19E | MISO
PC18E | SPCK
PC21E | NPCS0
PC22E | NPCS1

### Pin List for SPI Serial Flash Instance 5 (I/O Set 3)

Pin | Use
--- | ---
PB23E | MOSI
PB22E | MISO
PB21E | SPCK
PB24E | NPCS0
PB25E | NPCS1

### Pin List for SPI Serial Flash Instance 6 (I/O Set 1)

Pin | Use
--- | ---
PC28B | MOSI
PC29B | MISO
PC30B | SPCK
PC31B | NPCS0
PD0B | NPCS1

### Pin List for SPI Serial Flash Instance 6 (I/O Set 2)

Pin | Use
--- | ---
PD12B | MOSI
PD13B | MISO
PD14B | SPCK
PD15B | NPCS0
PD16B | NPCS1

### Pin List for SPI Serial Flash Instance 6 (I/O Set 3)

Pin | Use
--- | ---
PD21C | MOSI
PD22C | MISO
PD23C | SPCK
PD24C | NPCS0
PD25C | NPCS1

## NAND Flash Configuration

The following NAND Flash configurations are supported:

I/O Set | Bus Width
--- | ---
1, 2 | 8-bit, 16-bit

### Pin List for NAND Flash (I/O Set 1)

Pin | Use | Bus Width
--- | --- | ---
PA30B | NANDWE | 8-bit, 16-bit
PA31B | NCS3 | 8-bit, 16-bit
PB0B | NANDALE | 8-bit, 16-bit
PB1B | NANDCLE | 8-bit, 16-bit
PB2B | NANDOE | 8-bit, 16-bit
PC8B | NANDRDY | 8-bit, 16-bit
PA22B | D0 | 8-bit, 16-bit
PA23B | D1 | 8-bit, 16-bit
PA24B | D2 | 8-bit, 16-bit
PA25B | D3 | 8-bit, 16-bit
PA26B | D4 | 8-bit, 16-bit
PA27B | D5 | 8-bit, 16-bit
PA28B | D6 | 8-bit, 16-bit
PA29B | D7 | 8-bit, 16-bit
PB3B | D8 | 16-bit
PB4B | D9 | 16-bit
PB5B | D10 | 16-bit
PB6B | D11 | 16-bit
PB7B | D12 | 16-bit
PB8B | D13 | 16-bit
PB9B | D14 | 16-bit
PB10B | D15 | 16-bit

### Pin List for NAND Flash (I/O Set 2)

Pin | Use | Bus Width
--- | --- | ---
PA8F | NANDWE | 8-bit, 16-bit
PA9F | NCS3 | 8-bit, 16-bit
PA10F | NANDALE | 8-bit, 16-bit
PA11F | NANDCLE | 8-bit, 16-bit
PA12F | NANDOE | 8-bit, 16-bit
PA21F | NANDRDY | 8-bit, 16-bit
PA0F | D0 | 8-bit, 16-bit
PA1F | D1 | 8-bit, 16-bit
PA2F | D2 | 8-bit, 16-bit
PA3F | D3 | 8-bit, 16-bit
PA4F | D4 | 8-bit, 16-bit
PA5F | D5 | 8-bit, 16-bit
PA6F | D6 | 8-bit, 16-bit
PA7F | D7 | 8-bit, 16-bit
PA12F | D8 | 16-bit
PA13F | D9 | 16-bit
PA14F | D10 | 16-bit
PA15F | D11 | 16-bit
PA16F | D12 | 16-bit
PA17F | D13 | 16-bit
PA18F | D14 | 16-bit
PA18F | D15 | 16-bit

## QSPI Flash Configuration

The following QSPI Flash configurations are supported:

Instance | Peripheral | I/O Set
--- | --- | ---
0 | QSPI0 | 1, 2, 3
1 | QSPI1 | 1, 2, 3

### Pin List for QSPI Serial Flash Instance 0 (I/O Set 1)

Pin | Use
--- | ---
PA0B | SCK
PA1B | CS
PA2B | IO0
PA3B | IO1
PA4B | IO2
PA5B | IO3

### Pin List for QSPI Serial Flash Instance 0 (I/O Set 2)

Pin | Use
--- | ---
PA14C | SCK
PA15C | CS
PA16C | IO0
PA17C | IO1
PA18C | IO2
PA19C | IO3

### Pin List for QSPI Serial Flash Instance 0 (I/O Set 3)

Pin | Use
--- | ---
PA22F | SCK
PA23F | CS
PA24F | IO0
PA25F | IO1
PA26F | IO2
PA27F | IO3

### Pin List for QSPI Serial Flash Instance 1 (I/O Set 1)

Pin | Use | I/O Sets
--- | --- | ---
PA6B | SCK | 1
PA11B | CS | 1
PA7B | IO0 | 1
PA8B | IO1 | 1
PA9B | IO2 | 1
PA10B | IO3 | 1

### Pin List for QSPI Serial Flash Instance 1 (I/O Set 2)

Pin | Use | I/O Sets
--- | --- | ---
PB5D | SCK | 2
PB6D | CS | 2
PB7D | IO0 | 2
PB8D | IO1 | 2
PB9D | IO2 | 2
PB10D | IO3 | 2

### Pin List for QSPI Serial Flash Instance 1 (I/O Set 3)

Pin | Use | I/O Sets
--- | --- | ---
PB14E | SCK | 3
PB15E | CS | 3
PB16E | IO0 | 3
PB17E | IO1 | 3
PB18E | IO2 | 3
PB19E | IO3 | 3

## Property Documentation

extram : alias

Configuration for external RAM applet

See ExtRamConfig for a list of configurable properties.

nandflash : alias

Configuration for NAND Flash applet

See NANDFlashConfig for a list of configurable properties.

qspiflash : alias

Configuration for QSPI Flash applet

See QSPIFlashConfig for a list of configurable properties.

sdmmc : alias

Configuration for SD/MMC applet

See SDMMCConfig for a list of configurable properties.

serial : alias

Configuration for applet serial console output

See SerialConfig for a list of configurable properties.

serialflash : alias

Configuration for SPI Serial Flash applet

See SerialFlashConfig for a list of configurable properties.