Home ·

# SAMV71Config QML Type

Contains configuration values for a SAME70/S70/V70/V71 device. More...

Import Statement: | import SAMBA.Device.SAMV71 3.2

- List of all members, including inherited members

## Properties

- extram : alias
- serial : alias

## Detailed Description

By default, no configuration values are set.

## Serial Console Configuration

The following serial console configurations are supported:

Instance | Peripheral | I/O Set | TX Pin
--- | --- | --- | ---
0 | UART0 | 1 | PA10A
1 | UART1 | 1 | PA4C
1 | UART1 | 2 | PA6C
1 | UART1 | 3 | PD26D
2 | UART2 | 1 | PD26C
3 | UART3 | 1 | PD30A
3 | UART3 | 2 | PD31B
4 | UART4 | 1 | PD3C
4 | UART4 | 2 | PD19C
5 | USART0 | 1 | PB1C
6 | USART1 | 1 | PB4D
7 | USART2 | 1 | PD16B

## External RAM

The following external RAM configurations are supported:

Preset | Type | Model | Size
--- | --- | --- | ---
6 | SDRAM | IS42S16100E | 2MB
7 | SDRAM | W981216BH | 2MB
10 | SDRAM | AS4C16M16SA | 32MB

## Property Documentation

extram : alias

Configuration for External RAM applet

See ExtRamConfig for a list of configurable properties.

serial : alias

Configuration for applet serial console output

See SerialConfig for a list of configurable properties.